**LxT1-SE Final Checklist**

|  |  |  |
| --- | --- | --- |
| Instrument Type: | Preamplifier: | Microphone: |
| [x]  LxT | [x]  PRMLxT1L  |   |
| S/N  | S/N  | S/N  |

|  |  |
| --- | --- |
| Customer:  | Order Number:  |

 **Technician**

[ ]  Program model and serial number, and assign preamp **Standard Options**

[ ]  Place serial number label on back of the unit [x]  1/1 Octave (OB1)

[ ]  Passes production tests [x]  1/3 Octave (OB3)

[ ]  Keys tested [x]  Time History (LOG)

[ ]  LCD contrast and back light [x]  Community Noise (CN)

[ ]  AC/DC out, [x]  Measurement History (ENV)

[ ]  Performed acoustic test

[ ]  Format / Restore Defaults

[ ]  Program the options and set the date and time (D0001.8307)

[ ]  LxT-SE badge on the front of the unit

[ ]  Certificate of Calibration and Conformance printed and signed

[ ]  Calibration sticker placed in battery compartment

[ ]  Information entered into the database

 Select Flash Size:

 **Inspection**

[ ]  Calibrate with the customer’s microphone and save when prompted

[ ]  Check certification dates and manufacture date

[ ]  Verify the options programmed into the unit

[ ]  Technician Final Inspection slip

|  |  |  |
| --- | --- | --- |
| A770.01 REV.:  | Firmware version:  | Test station:  **METCAL** |

|  |  |  |  |
| --- | --- | --- | --- |
| Technician: |  | Date: |  |
| Materials Control: |  | Date: |  |
| Inspection: |  | Date: |  |