**LxT1-SE Final Checklist**

|  |  |  |
| --- | --- | --- |
| Instrument Type: | Preamplifier: | Microphone: |
| LxT | PRMLxT1L |  |
| S/N | S/N | S/N |

|  |  |
| --- | --- |
| Customer: | Order Number: |

**Technician**

Program model and serial number, and assign preamp **Standard Options**

Place serial number label on back of the unit  1/1 Octave (OB1)

Passes production tests  1/3 Octave (OB3)

Keys tested  Time History (LOG)

LCD contrast and back light  Community Noise (CN)

AC/DC out,  Measurement History (ENV)

Performed acoustic test

Format / Restore Defaults

Program the options and set the date and time (D0001.8307)

LxT-SE badge on the front of the unit

Certificate of Calibration and Conformance printed and signed

Calibration sticker placed in battery compartment

Information entered into the database

Select Flash Size:

**Inspection**

Calibrate with the customer’s microphone and save when prompted

Check certification dates and manufacture date

Verify the options programmed into the unit

Technician Final Inspection slip

|  |  |  |
| --- | --- | --- |
| A770.01 REV.: | Firmware version: | Test station:  **METCAL** |

|  |  |  |  |
| --- | --- | --- | --- |
| Technician: |  | Date: |  |
| Materials Control: |  | Date: |  |
| Inspection: |  | Date: |  |