**SHIPPED ATEX UNITS MONTH / YEAR:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **703+** | | **705+** | | **706RC** | |
| **#** | **DATE** | **SN** | **DATE** | **SN** | **DATE** | **SN** |
| **1** |  |  |  |  |  |  |
| **2** |  |  |  |  |  |  |
| **3** |  |  |  |  |  |  |
| **4** |  |  |  |  |  |  |
| **5** |  |  |  |  |  |  |
| **6** |  |  |  |  |  |  |
| **7** |  |  |  |  |  |  |
| **8** |  |  |  |  |  |  |
| **9** |  |  |  |  |  |  |
| **10** |  |  |  |  |  |  |
| **11** |  |  |  |  |  |  |
| **12** |  |  |  |  |  |  |
| **13** |  |  |  |  |  |  |
| **14** |  |  |  |  |  |  |
| **15** |  |  |  |  |  |  |
| **16** |  |  |  |  |  |  |
| **17** |  |  |  |  |  |  |
| **18** |  |  |  |  |  |  |
| **19** |  |  |  |  |  |  |
| **20** |  |  |  |  |  |  |
| **21** |  |  |  |  |  |  |
| **22** |  |  |  |  |  |  |
| **23** |  |  |  |  |  |  |
| **24** |  |  |  |  |  |  |
| **25** |  |  |  |  |  |  |
| **26** |  |  |  |  |  |  |
| **27** |  |  |  |  |  |  |
| **28** |  |  |  |  |  |  |
| **29** |  |  |  |  |  |  |
| **30** |  |  |  |  |  |  |
| **31** |  |  |  |  |  |  |
| **32** |  |  |  |  |  |  |
| **33** |  |  |  |  |  |  |
| **34** |  |  |  |  |  |  |
| **35** |  |  |  |  |  |  |
| **36** |  |  |  |  |  |  |
| **TOTALS** | |  |  |  |  |  |

**Instructions:**

**1- As each ATEX unit is shipped, log the date & serial number under the applicable model.**

**2- Do not mix months or years on the same page of the log.**

**3- Logs are reviewed at the time of the vertical audit by QA.**

**4- Following the review, the logs are removed from the clip board and stapled to the QA report, and submitted to Document Control.**

**5- The log and audit report are maintained in Document Control for a minimum of ten years from the date of audit.**