# Microelectronics

* Dress Code
	+ No soiled foot wear
	+ White coat buttoned all the way to top
	+ Personal garments tucked into white coat
	+ White coats should not be stored (unbagged), worn outside of, or removed from clean room/gowning room unless going out for cleaning
* Clean Room
	+ No Eating or Drinking in clean room, (chewing gum and hard candy is allowed if not stored in the cleanroom)
	+ Pass from the gowning area to the clean area slowly to reduce migration of particles between areas
	+ Anything entering the clean room should be wiped down to reduce contaminants from entering
	+ Do not use pencils or erasers
	+ No liquids, solvents, chemicals, or aerosols unless needed for production
	+ No cosmetics or personal grooming aids

Paper should not enter the clean room unless necessary. If on an ESD work surface, it should be placed in a ESD sleeve and remain in the sleeve except when writing on or turning a page.

# Microphones

* Dress Code
	+ No jewelry that can puncture garments or gloves
	+ No soiled foot wear
	+ No hat (including baseball caps) unless covered with a polypropylene clean room bouffant cap.
	+ No shorts or pants that expose any part of the leg
	+ White coat buttoned all the way to top
	+ Personal garments tucked into white coat
		- White coats with non-cuffed sleeves must be buttoned
		- Hoods and shirt collars/ turtleneck sweaters should remain covered by coat.
	+ White coats should not be stored (unbagged), worn outside of, or removed from clean room/gowning room unless going out for cleaning
* Clean Room
	+ No Eating or Drinking in clean room, (including chewing gum, hard candy or tobacco)
	+ Pass from the gowning area to the clean area slowly to reduce migration of particles between areas
	+ Anything entering the clean room should be wiped down to reduce contaminants from entering
	+ Do not use pencils or erasers
	+ No cosmetics or personal grooming aids

Paper should not enter the clean room unless necessary. If necessary, it should be placed in a sleeve and remain in the sleeve except when turning a page.

**Engine Sensor room**

* Dress Code
	+ No soiled foot wear
	+ White coat buttoned all the way to top
	+ Personal garments tucked into white coat.
	+ White coats should not be stored (unbagged), worn outside of, or removed from clean area unless going out for cleaning.
* Clean Area
	+ No Eating in clean area, (chewing gum and hard candy is allowed if not stored in the clean area)
	+ Pass through the door slowly to reduce migration of particles from outside
	+ Anything entering the clean area should be wiped down to reduce contaminants from entering
	+ Do not use pencils or erasers
	+ No liquids, solvents, chemicals, or aerosols unless needed for production
	+ No cosmetics or personal grooming aids

Paper should not enter the clean area unless necessary. If on an ESD work surface, it should be placed in a ESD sleeve and remain in the sleeve except when writing on or turning a page.